**Mobile Bluetooth Player User Manual**

Thank you for using this mobile Bluetooth player. This player features the following functions:

1. Simple operation and powerful sound effects, integrating radio, Bluetooth, and audio input functions.
2. Highly compatible and widely applicable; suitable for various mobile phones and can be used with phones, TVs, or other audio devices.
3. True stereo channel output enhances the dynamic feel of entertainment and leisure.
4. Widely used in swimming pools, bathtubs of various sizes, saunas/steam rooms, and outdoor pavilions.

**1. Panel Buttons:**

1. ▶▶ (Next Track)
2. FM/AUX/Bluetooth button (Menu function: switches between Radio, Bluetooth, and AUX)
3. ◀◀ (Previous Track)
4. VOL+ button (Increase volume)
5. VOL– button (Decrease volume)
6. Indicator lights:
 - Blue light on: Bluetooth mode
 - Green light on: AUX mode
 - Red light on: Radio mode

**2. Connection Terminals:**

1. DC12V5A power cord (inner positive, outer negative), 30 cm long × 1
2. AUX audio input cables for left and right channels, 30 cm long each × 1
3. Audio output cables for left and right channels, 30 cm long each × 1
4. Radio antenna, 1 meter long × 1

**3. Operating Instructions:**

1. **Power Button:**
 After powering on, the panel indicator shows a blue light, entering Bluetooth mode.
 Long-press the FM/AUX/Bluetooth button:
 - Blue light off, green light on → enters AUX mode
 - Green light off, red light on → enters FM radio mode
 Continue long-pressing to cycle through the modes.
2. **FM/AUX/Bluetooth Button:**  1) When in Bluetooth mode (blue light), pair with your phone (device name: XKD-01). After pairing, play music from your phone.
  Use ◀◀/▶▶ to select tracks, VOL+/VOL– to adjust volume.

 2) In FM radio mode (red light), press the FM/AUX/Bluetooth button once to automatically search and store radio stations.
  Use ◀◀/▶▶ to select radio channels, VOL+/VOL– to adjust volume.

 3) In AUX mode (green light), play music from your phone via AUX input.
  Use VOL+/VOL– to adjust volume.

**4. Basic Specifications:**

1. Left and right channel output power: 2 × 10W
2. Power supply: DC 12V 5A

**5. Compatible Products:**

1. 2-inch speakers, 2 × 4(8)Ω 3W / 3-inch speakers, 2 × 4(8)Ω 10W (optional)
2. DC 12V 8.5A dual-output power supply (can connect to both the player and TV or other audio devices)